Questions for Ed Stott

* If voltage source was defined between 0 and N00X, is that a “-1” at the corresponding node, followed by 0s for the entire row?
* Do voltage sources connected to ground replace their rows and columns with a 0, or just the row?
* Is the current vector solely made up of currents or known values?